{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"merged":[[0,0,0,3],[1,0,1,3],[3,0,8,0],[3,1,8,1],[9,0,13,0],[9,1,13,1],[14,0,15,0],[14,1,15,1],[17,0,19,0],[17,1,19,1],[20,0,22,0],[20,1,22,1],[23,0,28,0],[23,1,28,1],[29,0,34,0],[29,1,34,1],[32,3,33,3],[36,0,37,0],[36,1,37,1]],"flags":["formulas_cached_only"]}
["附件1"]
["连栋四季玻璃温室大棚"]
["序号","名称","备注","材质"]
[1,"温室主体骨架","主立柱：120mm*120mm*3.0mm","热镀锌"]
[null,null,"副立柱：120mm*120mm*3.0mm","热镀锌"]
[null,null,"抗风柱：50mm*50mm*2.0mm","热镀锌"]
[null,null,"横向桁架：上下玄50mm*50mm*2.5mm 角铁：3#","热浸锌",null,null,"    "]
[null,null,"水槽：2.0mm","热镀锌"]
[null,null,"四周围梁：50mm*50mm*2.0mm","热镀锌"]
[2,"标准件","M16*150"]
[null,null,"M12*70"]
[null,null,"M8*120"]
[null,null,"M8*70"]
[null,null,"钻尾丝：L19"]
[3,"冷凝水收集系统","0.6镀锌板","铝合金"]
[null,null,"集露槽挂钩","热镀锌"]
[4,"排水管","PVC排水管"]
[5,"顶通风系统","顶开窗电机","0.75kw"]
[null,null,"1米*2米铝合金天窗"]
[null,null,"传动系统"]
[6,"覆盖材料","顶部阳光板","8mm阳光板"]
[null,null,"四周玻璃","5+6+5中空玻璃"]
[null,null,"固定玻璃专用铝合金","氧化处理铝合金"]
[7,"内保温及四周内保温系统","遮阳拉幕电机：0.75kw"]
[null,null,"幕布：太空棉","加厚太空棉"]
[null,null,"齿轮齿条"]
[null,null,"幕线：透明"]
[null,null,"电动传动系统"]
[null,null,"齿条传动系统"]
[8,"降温系统","水帘：厚度100mm 镀锌边框","镀锌边框"]
[null,null,"供排水系统：PVC管件"]
[null,null,"水泵"]
[null,null,"外翻窗"]
[null,null,"传动系统"]
[null,null,"风机：1380*1380","不锈钢扇叶"]
[9,"门","肯德基推拉门"]
[10,"配电系统","配件柜"]
[null,null,"线管/电线电缆"]
[]
[]
[{"$nulls":5}," "]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}